Product Code/Ref | Description | Range | Language
8-450 | 2K Epoxy Primer wasserverdünnbar | Selemix Aqua | de-DE
8-460 | 2K Epoxy Decklack wasserverdünnbar | Selemix Aqua | de-DE
8-550 | 2K Polyurethan Decklack wasserverdünnbar | Selemix Aqua | de-DE
8-552 | 2K Polyurethan Decklack Extra wasserverdünnbar | Selemix Aqua | de-DE
2.704.8016 | 2K Epoxy Primer Grau wasserverdünnbar | Selemix Aqua | de-DE
2.704.8020 | 2K Epoxy Primer wasserverdünnbar | Selemix Aqua | de-DE
8-110 | 2K Polyurethan Direct Decklack wasserverdünnbar | Selemix Aqua | de-DE
8-553 | 2K Polyurethan Decklack, extramatt wasserverdünnbar | Selemix Aqua | de-DE
8-864 | 1K Decklack, Matt wasserverdünnbar | Selemix Aqua | de-DE
8-861 | 1K Decklack Extra wasserverdünnbar | Selemix Aqua | de-DE
8-551 | 2K Polyurethan Decklack, matt wasserverdünnbar | Selemix Aqua | de-DE
8-850 | 1K Primer schnelltrocknend wasserverdünnbar | Selemix Aqua | de-DE
7-020 | Kunstharz-Decklack, matt, streichbar | Selemix System | de-DE
7-080 | KH-Rostschutzgrund, streichbar | Selemix System | de-DE
7-110 | Acryl-Decklack | Selemix System | de-DE
7-310 | NC-Decklack | Selemix System | de-DE
7-330 | NC-Decklack, hochglänzend | Selemix System | de-DE
7-411 | Epoxy-Decklack, Strukturiert | Selemix System | de-DE
7-413 | Epoxy-Grundierung | Selemix System | de-DE
7-420 | Epoxy-Vinyl-Decklack | Selemix System | de-DE
7-511 | PUR-Decklack, matt | Selemix System | de-DE
7-513 | PUR-Decklack, strukturiert | Selemix System | de-DE
7-53X | PUR Direct - Decklack- Allgemein Informationen | Selemix System | de-DE
7-53X | PUR Direct - Decklack- VOC Konformer Härter | Selemix System | de-DE
7-611 | KH-Decklack, matt, schnelltrocknend | Selemix System | de-DE
7-620 | KH-Decklack, Eisenglimmer | Selemix System | de-DE
7-630 | KH-Urethan-Decklack | Selemix System | de-DE
7-648 | KH-Decklack, schnelltrocknend | Selemix System | de-DE
7-710 | KH-Einbrenn-Decklack, 120°C | Selemix System | de-DE
7-720 | Kunstharz Einbrennlack, matt, 120°C | Selemix System | de-DE
7-740 | KH-Einbrenn-Decklack, 80°C | Selemix System | de-DE
7-750 | KH-Einbrenn-Decklack, matt, 80°C | Selemix System | de-DE
7-810 | KH-Rostschutzgrund, schnelltrocknend | Selemix System | de-DE
7-820 | KH-Rostschutzgrundierung, | Selemix System | de-DE
7-861 | KH-Einschichtdecklack | Selemix System | de-DE
7-910 | KH-Chloralkyd-Decklack | Selemix System | de-DE
7-920 | Chlorkautschuk-Decklack | Selemix System | de-DE
6-540 | Additiv für Hammerschlageffekt-Decklacke | Selemix System | de-DE
7-030 | Kunstharz Decklack, streichbar | Selemix System | de-DE
7-083 | KH-Eischichtdecklack, streichbar | Selemix System | de-DE
7-120 | UHS-Acryl-Decklack | Selemix System | de-DE
7-320 | NC-Decklack, matt | Selemix System | de-DE
7-410 | Epoxy-Decklack | Selemix System | de-DE
7-412 | Epoxy-Decklack, matt | Selemix System | de-DE
7-414 | Epoxy-Vinyl-Grundierung | Selemix System | de-DE
7-510 | PUR-Decklack | Selemix System | de-DE
7-512 | PUR-Decklack, extra | Selemix System | de-DE
7-514 | PUR-Decklack für galvanisch | Selemix System | de-DE
7-53X | PUR Direct - Decklack- Standard Härter | Selemix System | de-DE
7-610 | KH-Decklack, schnelltrocknend | Selemix System | de-DE
NP1000 | PUR Decklack Standard Weiss | Selemix System | de-DE
2.704.0490 | 2K Zinc Rich Epoxy primer | Selemix System | de-DE
2.708.0900 | 1K Synthetik Primer | Selemix System | de-DE
2.776.0350/0600 | HT Decklack / Hoch-temperaturbeständing | Selemix System | de-DE
7-538/7-539 | PUR Direct - Decklack 80GL (VOC Konform Härter) | Selemix System | de-DE
7-538/7-539 | PUR Direct - Decklack 80GL | Selemix System | de-DE
6-560/6-561 | Microstrukturpulver - Additive | Selemix System | de-DE
6-580 | Streich-Additiv | Selemix System | de-DE
SPP2000 | Paint Performance Additiv | Selemix System | de-DE
SPP6970 | Electrostatik-Additiv | Selemix System | de-DE
7-130 | Acryl Decklack High Build | Selemix System | de-DE
2.704.0400 | Epoxy - Primer, beige | Selemix System | de-DE
2.704.0440 | High Build Epoxy - Primer, grau | Selemix System | de-DE
2.704.0480 | 2K Zinc Rich Epoxy Primer | Selemix System | de-DE
2.708.080X | 1K Primer | Selemix System | de-DE
2.705.020X | PUR Primer | Selemix System | de-DE